Description='LAN Interface'
Interface=eth1
Connection=ethernet
IP=static
Address=('10.20.0.1/24')
#Routes=('192.168.0.0/24 via 192.168.1.2')
#Gateway='141.76.90.1'
#DNS=('8.8.8.8')

## For IPv6 autoconfiguration
#IP6=stateless

## For IPv6 static address configuration
#IP6=static
#Address6=('1234:5678:9abc:def::1/64' '1234:3456::123/96')
#Routes6=('abcd::1234')
#Gateway6='1234:0:123::abcd'
